Telnet configuration in switch:

user SW1 password L00179213

enable password L00179213

conf t

line vty 0 4

password L00179213